


**BaoFeng DM-5R Programming Steps**

**NOTE:** The .rar files in this upgrading process are password protected. The password is: 123456

**Step 1:** In order to program the radio, connect the radio to your computer using the supplied programming cable in the USB drive and the programming cable input on the radio.


**Step 2:** Click START---CONTROL PANEL---DEVICE MANAGER—Port(COM)-- Prolific USB-to-Serial Comm Port (COM?).



**Step 3:** Open up the radio，Hold PTT, Rotate the On/Off knob, and you'll enter Developer Mode(IAP Mode). At this time the radio's display and keypad will light up, the screen will have a red light.





**Step 4:** Extract all of the compressed files into one folder, name that folder "DM-5R Prog". The .rar files are password protected. The password is: 123456.






**Step 5:** Delete the file titled "vsetting", Double-click to open "Hrvocoder Encryption" (the application [size approx. 750 KB], not the compressed file [size approx. 300KB]).








**Step 6:** Choose the port identified in step 2, choose the number 57600 from the drop down list. Click




At this time you'll see the following prompt: 。


**Step 7:** On the following menu, Choose


Choose the destination folder you created from the extraction in Step 4 "DM-5R Prog". From that folder, select the document ending in .bin

You will then see the following prompt: . At this time, make sure the radio's screen and keypad are lit up. After the screen turns red, Click Upgrade.Press OK.




Wait until the upgrade is 100% complete, you'll see the following in the bottom right corner:.


**Step 7:** turn off your radio, unplug the programming cable, close the cover to the programming input on the radio. 

Once more, programming cable connected to radio, start the radio normally, don't push PTT. Open this software, Open the port.

Clickto create an Excel Spreadsheet. Name this spreadsheet "DM-5R Spread". Change ONLY the name, keep the format the same.




Once more press




After opening, you'll see the following prompt in the bottom left corner:

ClickYou'll see the following prompt: 


Inside the excel spreadsheet that was just created, you'll see

Email us with your ID number. We will help you obtain a Key Value.

After we send you the Key Value, enter the Key Value into the "DM-5R Spread" Excel Spreadsheet from before.




Once again connect the programming cable to the radio, turn on the radio normally, not holding PTT. Open the software, Open the port.



Choose OPEN EXCEL. Select the Excel Spreadsheet you created before, named "DM-5R Spread".





After opening you'll see the prompt: 

Finally click: . You've reached the end of your update, once more disconnect the programming cable. Turn off the radio, next time you turn on the radio you can use it normally.

